# Static Call Graph for image f429_i2c\f429_i2c.axf

#<CALLGRAPH># ARM Linker, 5060750: Last Updated: Thu Jun 29 08:55:56 2023

### Maximum Stack Usage = 712 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ zam6218_demo_entry ⇒ zam6218_get_temp ⇒ __zam6218_read_data ⇒ HAL_I2C_Mem_Read ⇒ I2C_RequestMemoryRead ⇒ I2C_WaitOnMasterAddressFlagUntilTimeout

### Mutually Recursive functions

- ADC_IRQHandler ⇒ ADC_IRQHandler

  ### Function Pointers

  - ADC_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - BusFault_Handler from stm32f4xx_it.o(i.BusFault_Handler) referenced from startup_stm32f429xx.o(RESET)
  - CAN1_RX0_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - CAN1_RX1_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - CAN1_SCE_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - CAN1_TX_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - CAN2_RX0_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - CAN2_RX1_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - CAN2_SCE_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - CAN2_TX_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - DCMI_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - DMA1_Stream0_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - DMA1_Stream1_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - DMA1_Stream2_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - DMA1_Stream3_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - DMA1_Stream4_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - DMA1_Stream5_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - DMA1_Stream6_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - DMA1_Stream7_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - DMA2D_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - DMA2_Stream0_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - DMA2_Stream1_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - DMA2_Stream2_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - DMA2_Stream3_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - DMA2_Stream4_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - DMA2_Stream5_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - DMA2_Stream6_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - DMA2_Stream7_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - DebugMon_Handler from stm32f4xx_it.o(i.DebugMon_Handler) referenced from startup_stm32f429xx.o(RESET)
  - ETH_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - ETH_WKUP_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - EXTI0_IRQHandler from stm32f4xx_it.o(i.EXTI0_IRQHandler) referenced from startup_stm32f429xx.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - EXTI2_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - EXTI3_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - FLASH_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - FMC_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - FPU_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - HASH_RNG_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - HardFault_Handler from stm32f4xx_it.o(i.HardFault_Handler) referenced from startup_stm32f429xx.o(RESET)
  - I2C1_ER_IRQHandler from stm32f4xx_it.o(i.I2C1_ER_IRQHandler) referenced from startup_stm32f429xx.o(RESET)
  - I2C1_EV_IRQHandler from stm32f4xx_it.o(i.I2C1_EV_IRQHandler) referenced from startup_stm32f429xx.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - I2C3_ER_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - I2C3_EV_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - I2C_DMAAbort from stm32f4xx_hal_i2c.o(i.I2C_DMAAbort) referenced from stm32f4xx_hal_i2c.o(i.I2C_ITError)
  - I2C_DMAAbort from stm32f4xx_hal_i2c.o(i.I2C_DMAAbort) referenced from stm32f4xx_hal_i2c.o(i.I2C_Slave_STOPF)
  - LTDC_ER_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - LTDC_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - MemManage_Handler from stm32f4xx_it.o(i.MemManage_Handler) referenced from startup_stm32f429xx.o(RESET)
  - NMI_Handler from stm32f4xx_it.o(i.NMI_Handler) referenced from startup_stm32f429xx.o(RESET)
  - OTG_FS_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - OTG_FS_WKUP_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - OTG_HS_EP1_IN_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - OTG_HS_EP1_OUT_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - OTG_HS_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - OTG_HS_WKUP_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - PVD_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - PendSV_Handler from stm32f4xx_it.o(i.PendSV_Handler) referenced from startup_stm32f429xx.o(RESET)
  - RCC_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - RTC_Alarm_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - RTC_WKUP_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - Reset_Handler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - SAI1_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - SDIO_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - SPI1_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - SPI2_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - SPI3_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - SPI4_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - SPI5_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - SPI6_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - SVC_Handler from stm32f4xx_it.o(i.SVC_Handler) referenced from startup_stm32f429xx.o(RESET)
  - SysTick_Handler from stm32f4xx_it.o(i.SysTick_Handler) referenced from startup_stm32f429xx.o(RESET)
  - SystemInit from system_stm32f4xx.o(i.SystemInit) referenced from startup_stm32f429xx.o(.text)
  - TAMP_STAMP_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - TIM1_BRK_TIM9_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - TIM1_TRG_COM_TIM11_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - TIM1_UP_TIM10_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - TIM2_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - TIM3_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - TIM4_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - TIM5_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - TIM6_DAC_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - TIM7_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - TIM8_BRK_TIM12_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - TIM8_CC_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - TIM8_TRG_COM_TIM14_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - TIM8_UP_TIM13_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - UART4_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - UART5_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - UART7_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - UART8_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - UART_DMAAbortOnError from stm32f4xx_hal_uart.o(i.UART_DMAAbortOnError) referenced from stm32f4xx_hal_uart.o(i.HAL_UART_IRQHandler)
  - USART1_IRQHandler from stm32f4xx_it.o(i.USART1_IRQHandler) referenced from startup_stm32f429xx.o(RESET)
  - USART2_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - USART3_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - USART6_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - UsageFault_Handler from stm32f4xx_it.o(i.UsageFault_Handler) referenced from startup_stm32f429xx.o(RESET)
  - WWDG_IRQHandler from startup_stm32f429xx.o(.text) referenced from startup_stm32f429xx.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_stm32f429xx.o(.text)
  - _sputc from printfa.o(i._sputc) referenced from printfa.o(i.__0sprintf)
  - main from main.o(i.main) referenced from entry9a.o(.ARM.Collect$$$$0000000B)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

  __rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000D))

  __rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$0000000F))

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  ADC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Calls]

  - >> ADC_IRQHandler
  [Called By]
  - >> ADC_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f429xx.o(RESET)

  CAN1_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  CAN2_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  CAN2_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  CAN2_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  CAN2_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  DCMI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  DMA1_Stream0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  DMA1_Stream1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  DMA1_Stream2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  DMA1_Stream3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  DMA1_Stream4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  DMA1_Stream5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  DMA1_Stream6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  DMA1_Stream7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  DMA2D_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  DMA2_Stream0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  DMA2_Stream1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  DMA2_Stream2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  DMA2_Stream3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  DMA2_Stream4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  DMA2_Stream5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  DMA2_Stream6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  DMA2_Stream7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  ETH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  ETH_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  FMC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  FPU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  HASH_RNG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  I2C3_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  I2C3_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  LTDC_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  LTDC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  OTG_FS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  OTG_FS_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  OTG_HS_EP1_IN_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  OTG_HS_EP1_OUT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  OTG_HS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  OTG_HS_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  RTC_Alarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  RTC_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  SAI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  SDIO_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  SPI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  SPI5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  SPI6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  TAMP_STAMP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  TIM1_BRK_TIM9_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  TIM1_TRG_COM_TIM11_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  TIM1_UP_TIM10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  TIM5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  TIM6_DAC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  TIM7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  TIM8_BRK_TIM12_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  TIM8_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  TIM8_TRG_COM_TIM14_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  TIM8_UP_TIM13_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  UART4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  UART5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  UART7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  UART8_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  USART6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  __aeabi_uldivmod (Thumb, 98 bytes, Stack size 40 bytes, uldiv.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = __aeabi_uldivmod
  [Calls]
  - >> __aeabi_llsr
  - >> __aeabi_llsl
  [Called By]
  - >> _printf_core
  - >> _fp_digits
  - >> HAL_RCC_GetSysClockFreq
  - >> UART_SetConfig

  __aeabi_memcpy (Thumb, 36 bytes, Stack size 0 bytes, memcpya.o(.text), UNUSED)

  __aeabi_memcpy4 (Thumb, 0 bytes, Stack size 0 bytes, memcpya.o(.text))
  [Called By]

  - >> main

  __aeabi_memcpy8 (Thumb, 0 bytes, Stack size 0 bytes, memcpya.o(.text), UNUSED)

  __aeabi_memset (Thumb, 14 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)
  [Called By]

  - >> _memset$wrapper
  - >> __aeabi_memclr

  __aeabi_memset4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memset8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memclr (Thumb, 4 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  __aeabi_memclr4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text))
  [Called By]

  - >> zam6218_get_temp
  - >> HAL_UART_MspInit
  - >> HAL_I2C_MspInit
  - >> zam6218_demo_entry
  - >> SystemClock_Config
  - >> MX_GPIO_Init

  __aeabi_memclr8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  _memset$wrapper (Thumb, 18 bytes, Stack size 8 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  strlen (Thumb, 14 bytes, Stack size 0 bytes, strlen.o(.text))
  [Called By]

  - >> ptintf_info

  __aeabi_f2d (Thumb, 38 bytes, Stack size 0 bytes, f2d.o(.text))
  [Called By]

  - >> zam6218_demo_entry

  __aeabi_uidiv (Thumb, 0 bytes, Stack size 12 bytes, uidiv.o(.text), UNUSED)

  __aeabi_uidivmod (Thumb, 44 bytes, Stack size 12 bytes, uidiv.o(.text), UNUSED)
  [Called By]

  - >> _printf_core

  __aeabi_llsl (Thumb, 30 bytes, Stack size 0 bytes, llshl.o(.text))
  [Called By]

  - >> _double_epilogue
  - >> __aeabi_dadd
  - >> __aeabi_d2ulz
  - >> __aeabi_uldivmod

  _ll_shift_l (Thumb, 0 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)

  __aeabi_llsr (Thumb, 32 bytes, Stack size 0 bytes, llushr.o(.text))
  [Called By]

  - >> _double_epilogue
  - >> __aeabi_d2ulz
  - >> __aeabi_uldivmod

  _ll_ushift_r (Thumb, 0 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)

  __I$use$fp (Thumb, 0 bytes, Stack size 48 bytes, iusefp.o(.text), UNUSED)

  __aeabi_dadd (Thumb, 322 bytes, Stack size 48 bytes, dadd.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_lasr
  - >> _double_round
  - >> _double_epilogue
  - >> __aeabi_llsl
  [Called By]
  - >> __aeabi_drsub
  - >> __aeabi_dsub
  - >> _fp_digits

  __aeabi_dsub (Thumb, 6 bytes, Stack size 0 bytes, dadd.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_dadd

  __aeabi_drsub (Thumb, 6 bytes, Stack size 0 bytes, dadd.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_dadd

  __aeabi_dmul (Thumb, 228 bytes, Stack size 48 bytes, dmul.o(.text), UNUSED)
  [Calls]

  - >> _double_epilogue
  [Called By]
  - >> _fp_digits

  __aeabi_ddiv (Thumb, 222 bytes, Stack size 32 bytes, ddiv.o(.text), UNUSED)
  [Calls]

  - >> _double_round
  [Called By]
  - >> _fp_digits

  __aeabi_d2ulz (Thumb, 48 bytes, Stack size 0 bytes, dfixul.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_llsr
  - >> __aeabi_llsl
  [Called By]
  - >> _fp_digits

  __aeabi_cdrcmple (Thumb, 48 bytes, Stack size 0 bytes, cdrcmple.o(.text), UNUSED)
  [Called By]

  - >> _fp_digits

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  __aeabi_lasr (Thumb, 36 bytes, Stack size 0 bytes, llsshr.o(.text), UNUSED)
  [Called By]

  - >> __aeabi_dadd

  _ll_sshift_r (Thumb, 0 bytes, Stack size 0 bytes, llsshr.o(.text), UNUSED)

  _double_round (Thumb, 30 bytes, Stack size 8 bytes, depilogue.o(.text), UNUSED)
  [Called By]

  - >> _double_epilogue
  - >> __aeabi_ddiv
  - >> __aeabi_dadd

  _double_epilogue (Thumb, 156 bytes, Stack size 32 bytes, depilogue.o(.text), UNUSED)
  [Calls]

  - >> _double_round
  - >> __aeabi_llsr
  - >> __aeabi_llsl
  [Called By]
  - >> __aeabi_dmul
  - >> __aeabi_dadd

  BusFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.BusFault_Handler))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.DebugMon_Handler))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  EXTI0_IRQHandler (Thumb, 10 bytes, Stack size 8 bytes, stm32f4xx_it.o(i.EXTI0_IRQHandler))
  [Stack]

  - Max Depth = 16
  - Call Chain = EXTI0_IRQHandler ⇒ HAL_GPIO_EXTI_IRQHandler
  [Calls]
  - >> HAL_GPIO_EXTI_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f429xx.o(RESET)

  Error_Handler (Thumb, 6 bytes, Stack size 0 bytes, main.o(i.Error_Handler))
  [Called By]

  - >> SystemClock_Config
  - >> MX_USART1_UART_Init
  - >> MX_I2C1_Init

  HAL_DMA_Abort (Thumb, 170 bytes, Stack size 16 bytes, stm32f4xx_hal_dma.o(i.HAL_DMA_Abort))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_DMA_Abort
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> HAL_UART_IRQHandler

  HAL_DMA_Abort_IT (Thumb, 40 bytes, Stack size 0 bytes, stm32f4xx_hal_dma.o(i.HAL_DMA_Abort_IT))
  [Called By]

  - >> I2C_Slave_STOPF
  - >> I2C_ITError
  - >> HAL_UART_IRQHandler

  HAL_DMA_GetState (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_hal_dma.o(i.HAL_DMA_GetState))
  [Called By]

  - >> I2C_Slave_STOPF

  HAL_GPIO_EXTI_Callback (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_hal_gpio.o(i.HAL_GPIO_EXTI_Callback))
  [Called By]

  - >> HAL_GPIO_EXTI_IRQHandler

  HAL_GPIO_EXTI_IRQHandler (Thumb, 24 bytes, Stack size 8 bytes, stm32f4xx_hal_gpio.o(i.HAL_GPIO_EXTI_IRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_GPIO_EXTI_IRQHandler
  [Calls]
  - >> HAL_GPIO_EXTI_Callback
  [Called By]
  - >> EXTI0_IRQHandler

  HAL_GPIO_Init (Thumb, 490 bytes, Stack size 24 bytes, stm32f4xx_hal_gpio.o(i.HAL_GPIO_Init))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_GPIO_Init
  [Called By]
  - >> HAL_UART_MspInit
  - >> HAL_I2C_MspInit

  HAL_GetTick (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_hal.o(i.HAL_GetTick))
  [Called By]

  - >> I2C_WaitOnTXEFlagUntilTimeout
  - >> I2C_WaitOnRXNEFlagUntilTimeout
  - >> I2C_WaitOnMasterAddressFlagUntilTimeout
  - >> I2C_WaitOnFlagUntilTimeout
  - >> I2C_WaitOnBTFFlagUntilTimeout
  - >> HAL_I2C_Mem_Write
  - >> HAL_I2C_Mem_Read
  - >> HAL_UART_Transmit
  - >> HAL_RCC_OscConfig
  - >> HAL_RCC_ClockConfig
  - >> HAL_DMA_Abort
  - >> UART_WaitOnFlagUntilTimeout

  HAL_I2CEx_ConfigAnalogFilter (Thumb, 76 bytes, Stack size 0 bytes, stm32f4xx_hal_i2c_ex.o(i.HAL_I2CEx_ConfigAnalogFilter))
  [Called By]

  - >> MX_I2C1_Init

  HAL_I2CEx_ConfigDigitalFilter (Thumb, 80 bytes, Stack size 8 bytes, stm32f4xx_hal_i2c_ex.o(i.HAL_I2CEx_ConfigDigitalFilter))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_I2CEx_ConfigDigitalFilter
  [Called By]
  - >> MX_I2C1_Init

  HAL_I2C_AbortCpltCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_hal_i2c.o(i.HAL_I2C_AbortCpltCallback))
  [Called By]

  - >> I2C_ITError
  - >> I2C_DMAAbort

  HAL_I2C_AddrCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_hal_i2c.o(i.HAL_I2C_AddrCallback))
  [Called By]

  - >> I2C_Slave_ADDR

  HAL_I2C_ER_IRQHandler (Thumb, 212 bytes, Stack size 40 bytes, stm32f4xx_hal_i2c.o(i.HAL_I2C_ER_IRQHandler))
  [Stack]

  - Max Depth = 64
  - Call Chain = HAL_I2C_ER_IRQHandler ⇒ I2C_ITError
  [Calls]
  - >> I2C_Slave_AF
  - >> I2C_ITError
  [Called By]
  - >> I2C1_ER_IRQHandler

  HAL_I2C_EV_IRQHandler (Thumb, 468 bytes, Stack size 32 bytes, stm32f4xx_hal_i2c.o(i.HAL_I2C_EV_IRQHandler))
  [Stack]

  - Max Depth = 72
  - Call Chain = HAL_I2C_EV_IRQHandler ⇒ I2C_Slave_STOPF ⇒ I2C_ITError
  [Calls]
  - >> I2C_Slave_STOPF
  - >> I2C_Slave_ADDR
  - >> I2C_SlaveTransmit_TXE
  - >> I2C_SlaveTransmit_BTF
  - >> I2C_SlaveReceive_RXNE
  - >> I2C_SlaveReceive_BTF
  - >> I2C_MemoryTransmit_TXE_BTF
  - >> I2C_Master_SB
  - >> I2C_Master_ADDR
  - >> I2C_Master_ADD10
  - >> I2C_MasterTransmit_TXE
  - >> I2C_MasterTransmit_BTF
  - >> I2C_MasterReceive_RXNE
  - >> I2C_MasterReceive_BTF
  - >> I2C_ConvertOtherXferOptions
  [Called By]
  - >> I2C1_EV_IRQHandler

  HAL_I2C_ErrorCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_hal_i2c.o(i.HAL_I2C_ErrorCallback))
  [Called By]

  - >> I2C_MasterReceive_RXNE
  - >> I2C_ITError
  - >> I2C_DMAAbort

  HAL_I2C_Init (Thumb, 446 bytes, Stack size 16 bytes, stm32f4xx_hal_i2c.o(i.HAL_I2C_Init))
  [Stack]

  - Max Depth = 96
  - Call Chain = HAL_I2C_Init ⇒ HAL_I2C_MspInit ⇒ HAL_NVIC_SetPriority ⇒ __NVIC_SetPriority
  [Calls]
  - >> HAL_I2C_MspInit
  - >> HAL_RCC_GetPCLK1Freq
  [Called By]
  - >> MX_I2C1_Init

  HAL_I2C_ListenCpltCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_hal_i2c.o(i.HAL_I2C_ListenCpltCallback))
  [Called By]

  - >> I2C_Slave_STOPF
  - >> I2C_Slave_AF
  - >> I2C_ITError

  HAL_I2C_MasterRxCpltCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_hal_i2c.o(i.HAL_I2C_MasterRxCpltCallback))
  [Called By]

  - >> I2C_MasterReceive_RXNE
  - >> I2C_MasterReceive_BTF

  HAL_I2C_MasterTxCpltCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_hal_i2c.o(i.HAL_I2C_MasterTxCpltCallback))
  [Called By]

  - >> I2C_MasterTransmit_TXE
  - >> I2C_MasterTransmit_BTF

  HAL_I2C_MemRxCpltCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_hal_i2c.o(i.HAL_I2C_MemRxCpltCallback))
  [Called By]

  - >> I2C_MasterReceive_RXNE
  - >> I2C_MasterReceive_BTF

  HAL_I2C_MemTxCpltCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_hal_i2c.o(i.HAL_I2C_MemTxCpltCallback))
  [Called By]

  - >> I2C_MemoryTransmit_TXE_BTF
  - >> I2C_MasterTransmit_TXE

  HAL_I2C_Mem_Read (Thumb, 744 bytes, Stack size 48 bytes, stm32f4xx_hal_i2c.o(i.HAL_I2C_Mem_Read))
  [Stack]

  - Max Depth = 104
  - Call Chain = HAL_I2C_Mem_Read ⇒ I2C_RequestMemoryRead ⇒ I2C_WaitOnMasterAddressFlagUntilTimeout
  [Calls]
  - >> I2C_WaitOnRXNEFlagUntilTimeout
  - >> I2C_WaitOnFlagUntilTimeout
  - >> I2C_RequestMemoryRead
  - >> HAL_GetTick
  [Called By]
  - >> __zam6218_read_data

  HAL_I2C_Mem_Write (Thumb, 348 bytes, Stack size 48 bytes, stm32f4xx_hal_i2c.o(i.HAL_I2C_Mem_Write))
  [Stack]

  - Max Depth = 104
  - Call Chain = HAL_I2C_Mem_Write ⇒ I2C_RequestMemoryWrite ⇒ I2C_WaitOnMasterAddressFlagUntilTimeout
  [Calls]
  - >> I2C_WaitOnTXEFlagUntilTimeout
  - >> I2C_WaitOnFlagUntilTimeout
  - >> I2C_WaitOnBTFFlagUntilTimeout
  - >> I2C_RequestMemoryWrite
  - >> HAL_GetTick
  [Called By]
  - >> __zam6218_write_data

  HAL_I2C_MspInit (Thumb, 156 bytes, Stack size 32 bytes, stm32f4xx_hal_msp.o(i.HAL_I2C_MspInit))
  [Stack]

  - Max Depth = 80
  - Call Chain = HAL_I2C_MspInit ⇒ HAL_NVIC_SetPriority ⇒ __NVIC_SetPriority
  [Calls]
  - >> HAL_NVIC_SetPriority
  - >> HAL_NVIC_EnableIRQ
  - >> HAL_GPIO_Init
  - >> __aeabi_memclr4
  [Called By]
  - >> HAL_I2C_Init

  HAL_I2C_SlaveRxCpltCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_hal_i2c.o(i.HAL_I2C_SlaveRxCpltCallback))
  [Called By]

  - >> I2C_Slave_STOPF
  - >> I2C_SlaveReceive_RXNE

  HAL_I2C_SlaveTxCpltCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_hal_i2c.o(i.HAL_I2C_SlaveTxCpltCallback))
  [Called By]

  - >> I2C_Slave_AF
  - >> I2C_SlaveTransmit_TXE

  HAL_IncTick (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_hal.o(i.HAL_IncTick))
  [Called By]

  - >> SysTick_Handler

  HAL_Init (Thumb, 54 bytes, Stack size 8 bytes, stm32f4xx_hal.o(i.HAL_Init))
  [Stack]

  - Max Depth = 72
  - Call Chain = HAL_Init ⇒ HAL_InitTick ⇒ HAL_NVIC_SetPriority ⇒ __NVIC_SetPriority
  [Calls]
  - >> HAL_MspInit
  - >> HAL_NVIC_SetPriorityGrouping
  - >> HAL_InitTick
  [Called By]
  - >> main

  HAL_InitTick (Thumb, 64 bytes, Stack size 16 bytes, stm32f4xx_hal.o(i.HAL_InitTick))
  [Stack]

  - Max Depth = 64
  - Call Chain = HAL_InitTick ⇒ HAL_NVIC_SetPriority ⇒ __NVIC_SetPriority
  [Calls]
  - >> HAL_NVIC_SetPriority
  - >> HAL_SYSTICK_Config
  [Called By]
  - >> HAL_RCC_ClockConfig
  - >> HAL_Init

  HAL_MspInit (Thumb, 68 bytes, Stack size 8 bytes, stm32f4xx_hal_msp.o(i.HAL_MspInit))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_MspInit
  [Called By]
  - >> HAL_Init

  HAL_NVIC_EnableIRQ (Thumb, 32 bytes, Stack size 0 bytes, stm32f4xx_hal_cortex.o(i.HAL_NVIC_EnableIRQ))
  [Called By]

  - >> HAL_UART_MspInit
  - >> HAL_I2C_MspInit

  HAL_NVIC_SetPriority (Thumb, 124 bytes, Stack size 40 bytes, stm32f4xx_hal_cortex.o(i.HAL_NVIC_SetPriority))
  [Stack]

  - Max Depth = 48
  - Call Chain = HAL_NVIC_SetPriority ⇒ __NVIC_SetPriority
  [Calls]
  - >> __NVIC_SetPriority
  - >> __NVIC_GetPriorityGrouping
  [Called By]
  - >> HAL_UART_MspInit
  - >> HAL_I2C_MspInit
  - >> HAL_InitTick

  HAL_NVIC_SetPriorityGrouping (Thumb, 32 bytes, Stack size 0 bytes, stm32f4xx_hal_cortex.o(i.HAL_NVIC_SetPriorityGrouping))
  [Called By]

  - >> HAL_Init

  HAL_RCC_ClockConfig (Thumb, 368 bytes, Stack size 16 bytes, stm32f4xx_hal_rcc.o(i.HAL_RCC_ClockConfig))
  [Stack]

  - Max Depth = 88
  - Call Chain = HAL_RCC_ClockConfig ⇒ HAL_RCC_GetSysClockFreq ⇒ __aeabi_uldivmod
  [Calls]
  - >> HAL_RCC_GetSysClockFreq
  - >> HAL_InitTick
  - >> HAL_GetTick
  [Called By]
  - >> SystemClock_Config

  HAL_RCC_GetHCLKFreq (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_hal_rcc.o(i.HAL_RCC_GetHCLKFreq))
  [Called By]

  - >> HAL_RCC_GetPCLK2Freq
  - >> HAL_RCC_GetPCLK1Freq

  HAL_RCC_GetPCLK1Freq (Thumb, 22 bytes, Stack size 4 bytes, stm32f4xx_hal_rcc.o(i.HAL_RCC_GetPCLK1Freq))
  [Stack]

  - Max Depth = 4
  - Call Chain = HAL_RCC_GetPCLK1Freq
  [Calls]
  - >> HAL_RCC_GetHCLKFreq
  [Called By]
  - >> HAL_I2C_Init
  - >> UART_SetConfig

  HAL_RCC_GetPCLK2Freq (Thumb, 22 bytes, Stack size 4 bytes, stm32f4xx_hal_rcc.o(i.HAL_RCC_GetPCLK2Freq))
  [Stack]

  - Max Depth = 4
  - Call Chain = HAL_RCC_GetPCLK2Freq
  [Calls]
  - >> HAL_RCC_GetHCLKFreq
  [Called By]
  - >> UART_SetConfig

  HAL_RCC_GetSysClockFreq (Thumb, 162 bytes, Stack size 32 bytes, stm32f4xx_hal_rcc.o(i.HAL_RCC_GetSysClockFreq))
  [Stack]

  - Max Depth = 72
  - Call Chain = HAL_RCC_GetSysClockFreq ⇒ __aeabi_uldivmod
  [Calls]
  - >> __aeabi_uldivmod
  [Called By]
  - >> HAL_RCC_ClockConfig

  HAL_RCC_OscConfig (Thumb, 1172 bytes, Stack size 24 bytes, stm32f4xx_hal_rcc.o(i.HAL_RCC_OscConfig))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_RCC_OscConfig
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> SystemClock_Config

  HAL_SYSTICK_Config (Thumb, 52 bytes, Stack size 16 bytes, stm32f4xx_hal_cortex.o(i.HAL_SYSTICK_Config))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_SYSTICK_Config ⇒ __NVIC_SetPriority
  [Calls]
  - >> __NVIC_SetPriority
  [Called By]
  - >> HAL_InitTick

  HAL_UARTEx_RxEventCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_hal_uart.o(i.HAL_UARTEx_RxEventCallback))
  [Called By]

  - >> HAL_UART_IRQHandler
  - >> UART_Receive_IT

  HAL_UART_ErrorCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_hal_uart.o(i.HAL_UART_ErrorCallback))
  [Called By]

  - >> HAL_UART_IRQHandler
  - >> UART_DMAAbortOnError

  HAL_UART_IRQHandler (Thumb, 586 bytes, Stack size 40 bytes, stm32f4xx_hal_uart.o(i.HAL_UART_IRQHandler))
  [Stack]

  - Max Depth = 56
  - Call Chain = HAL_UART_IRQHandler ⇒ HAL_DMA_Abort
  [Calls]
  - >> HAL_DMA_Abort
  - >> HAL_DMA_Abort_IT
  - >> HAL_UART_ErrorCallback
  - >> HAL_UARTEx_RxEventCallback
  - >> UART_Transmit_IT
  - >> UART_Receive_IT
  - >> UART_EndTransmit_IT
  - >> UART_EndRxTransfer
  [Called By]
  - >> USART1_IRQHandler

  HAL_UART_Init (Thumb, 114 bytes, Stack size 8 bytes, stm32f4xx_hal_uart.o(i.HAL_UART_Init))
  [Stack]

  - Max Depth = 88
  - Call Chain = HAL_UART_Init ⇒ HAL_UART_MspInit ⇒ HAL_NVIC_SetPriority ⇒ __NVIC_SetPriority
  [Calls]
  - >> HAL_UART_MspInit
  - >> UART_SetConfig
  [Called By]
  - >> MX_USART1_UART_Init

  HAL_UART_MspInit (Thumb, 140 bytes, Stack size 32 bytes, stm32f4xx_hal_msp.o(i.HAL_UART_MspInit))
  [Stack]

  - Max Depth = 80
  - Call Chain = HAL_UART_MspInit ⇒ HAL_NVIC_SetPriority ⇒ __NVIC_SetPriority
  [Calls]
  - >> HAL_NVIC_SetPriority
  - >> HAL_NVIC_EnableIRQ
  - >> HAL_GPIO_Init
  - >> __aeabi_memclr4
  [Called By]
  - >> HAL_UART_Init

  HAL_UART_RxCpltCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_hal_uart.o(i.HAL_UART_RxCpltCallback))
  [Called By]

  - >> UART_Receive_IT

  HAL_UART_Transmit (Thumb, 210 bytes, Stack size 40 bytes, stm32f4xx_hal_uart.o(i.HAL_UART_Transmit))
  [Stack]

  - Max Depth = 64
  - Call Chain = HAL_UART_Transmit ⇒ UART_WaitOnFlagUntilTimeout
  [Calls]
  - >> HAL_GetTick
  - >> UART_WaitOnFlagUntilTimeout
  [Called By]
  - >> ptintf_info

  HAL_UART_TxCpltCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_hal_uart.o(i.HAL_UART_TxCpltCallback))
  [Called By]

  - >> UART_EndTransmit_IT

  HardFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.HardFault_Handler))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 10 bytes, Stack size 8 bytes, stm32f4xx_it.o(i.I2C1_ER_IRQHandler))
  [Stack]

  - Max Depth = 72
  - Call Chain = I2C1_ER_IRQHandler ⇒ HAL_I2C_ER_IRQHandler ⇒ I2C_ITError
  [Calls]
  - >> HAL_I2C_ER_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f429xx.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 10 bytes, Stack size 8 bytes, stm32f4xx_it.o(i.I2C1_EV_IRQHandler))
  [Stack]

  - Max Depth = 80
  - Call Chain = I2C1_EV_IRQHandler ⇒ HAL_I2C_EV_IRQHandler ⇒ I2C_Slave_STOPF ⇒ I2C_ITError
  [Calls]
  - >> HAL_I2C_EV_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f429xx.o(RESET)

  MemManage_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.MemManage_Handler))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  NMI_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.NMI_Handler))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.PendSV_Handler))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.SVC_Handler))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  SysTick_Handler (Thumb, 8 bytes, Stack size 8 bytes, stm32f4xx_it.o(i.SysTick_Handler))
  [Stack]

  - Max Depth = 8
  - Call Chain = SysTick_Handler
  [Calls]
  - >> HAL_IncTick
  [Address Reference Count : 1]
  - startup_stm32f429xx.o(RESET)

  SystemClock_Config (Thumb, 148 bytes, Stack size 80 bytes, main.o(i.SystemClock_Config))
  [Stack]

  - Max Depth = 168
  - Call Chain = SystemClock_Config ⇒ HAL_RCC_ClockConfig ⇒ HAL_RCC_GetSysClockFreq ⇒ __aeabi_uldivmod
  [Calls]
  - >> HAL_RCC_OscConfig
  - >> HAL_RCC_ClockConfig
  - >> Error_Handler
  - >> __aeabi_memclr4
  [Called By]
  - >> main

  SystemInit (Thumb, 14 bytes, Stack size 0 bytes, system_stm32f4xx.o(i.SystemInit))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(.text)

  USART1_IRQHandler (Thumb, 10 bytes, Stack size 8 bytes, stm32f4xx_it.o(i.USART1_IRQHandler))
  [Stack]

  - Max Depth = 64
  - Call Chain = USART1_IRQHandler ⇒ HAL_UART_IRQHandler ⇒ HAL_DMA_Abort
  [Calls]
  - >> HAL_UART_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f429xx.o(RESET)

  UsageFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.UsageFault_Handler))
  [Address Reference Count : 1]

  - startup_stm32f429xx.o(RESET)

  __0sprintf (Thumb, 34 bytes, Stack size 24 bytes, printfa.o(i.__0sprintf), UNUSED)
  [Calls]

  - >> _sputc
  - >> _printf_core

  __1sprintf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0sprintf), UNUSED)

  __2sprintf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0sprintf))
  [Stack]

  - Max Depth = 24
  - Call Chain = __2sprintf
  [Called By]
  - >> zam6218_demo_entry

  __c89sprintf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0sprintf), UNUSED)

  sprintf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0sprintf), UNUSED)

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  delay_ms (Thumb, 28 bytes, Stack size 0 bytes, main.o(i.delay_ms))
  [Called By]

  - >> zam6218_demo_entry
  - >> main

  main (Thumb, 172 bytes, Stack size 160 bytes, main.o(i.main))
  [Stack]

  - Max Depth = 712
  - Call Chain = main ⇒ zam6218_demo_entry ⇒ zam6218_get_temp ⇒ __zam6218_read_data ⇒ HAL_I2C_Mem_Read ⇒ I2C_RequestMemoryRead ⇒ I2C_WaitOnMasterAddressFlagUntilTimeout
  [Calls]
  - >> zam6218_demo_entry
  - >> HAL_Init
  - >> ptintf_info
  - >> delay_ms
  - >> SystemClock_Config
  - >> MX_USART1_UART_Init
  - >> MX_I2C1_Init
  - >> MX_GPIO_Init
  - >> __aeabi_memcpy4
  [Address Reference Count : 1]
  - entry9a.o(.ARM.Collect$$$$0000000B)

  ptintf_info (Thumb, 28 bytes, Stack size 16 bytes, main.o(i.ptintf_info))
  [Stack]

  - Max Depth = 80
  - Call Chain = ptintf_info ⇒ HAL_UART_Transmit ⇒ UART_WaitOnFlagUntilTimeout
  [Calls]
  - >> HAL_UART_Transmit
  - >> strlen
  [Called By]
  - >> zam6218_demo_entry
  - >> main

  zam6218_config_set (Thumb, 46 bytes, Stack size 24 bytes, zam6218.o(i.zam6218_config_set))
  [Stack]

  - Max Depth = 168
  - Call Chain = zam6218_config_set ⇒ __zam6218_write_data ⇒ HAL_I2C_Mem_Write ⇒ I2C_RequestMemoryWrite ⇒ I2C_WaitOnMasterAddressFlagUntilTimeout
  [Calls]
  - >> __zam6218_write_data
  [Called By]
  - >> zam6218_demo_entry

  zam6218_demo_entry (Thumb, 366 bytes, Stack size 320 bytes, zam6218_demo_entry.o(i.zam6218_demo_entry))
  [Stack]

  - Max Depth = 552
  - Call Chain = zam6218_demo_entry ⇒ zam6218_get_temp ⇒ __zam6218_read_data ⇒ HAL_I2C_Mem_Read ⇒ I2C_RequestMemoryRead ⇒ I2C_WaitOnMasterAddressFlagUntilTimeout
  [Calls]
  - >> __aeabi_f2d
  - >> zam6218_get_temp
  - >> zam6218_config_set
  - >> ptintf_info
  - >> delay_ms
  - >> __2sprintf
  - >> __aeabi_memclr4
  [Called By]
  - >> main

  zam6218_get_temp (Thumb, 288 bytes, Stack size 88 bytes, zam6218.o(i.zam6218_get_temp))
  [Stack]

  - Max Depth = 232
  - Call Chain = zam6218_get_temp ⇒ __zam6218_read_data ⇒ HAL_I2C_Mem_Read ⇒ I2C_RequestMemoryRead ⇒ I2C_WaitOnMasterAddressFlagUntilTimeout
  [Calls]
  - >> __zam6218_reg_to_temp
  - >> __zam6218_read_data
  - >> __aeabi_memclr4
  [Called By]
  - >> zam6218_demo_entry

  ### Local Symbols

  MX_GPIO_Init (Thumb, 78 bytes, Stack size 32 bytes, main.o(i.MX_GPIO_Init))
  [Stack]

  - Max Depth = 32
  - Call Chain = MX_GPIO_Init
  [Calls]
  - >> __aeabi_memclr4
  [Called By]
  - >> main

  MX_I2C1_Init (Thumb, 76 bytes, Stack size 8 bytes, main.o(i.MX_I2C1_Init))
  [Stack]

  - Max Depth = 104
  - Call Chain = MX_I2C1_Init ⇒ HAL_I2C_Init ⇒ HAL_I2C_MspInit ⇒ HAL_NVIC_SetPriority ⇒ __NVIC_SetPriority
  [Calls]
  - >> HAL_I2C_Init
  - >> HAL_I2CEx_ConfigDigitalFilter
  - >> HAL_I2CEx_ConfigAnalogFilter
  - >> Error_Handler
  [Called By]
  - >> main

  MX_USART1_UART_Init (Thumb, 46 bytes, Stack size 8 bytes, main.o(i.MX_USART1_UART_Init))
  [Stack]

  - Max Depth = 96
  - Call Chain = MX_USART1_UART_Init ⇒ HAL_UART_Init ⇒ HAL_UART_MspInit ⇒ HAL_NVIC_SetPriority ⇒ __NVIC_SetPriority
  [Calls]
  - >> HAL_UART_Init
  - >> Error_Handler
  [Called By]
  - >> main

  __zam6218_read_data (Thumb, 66 bytes, Stack size 40 bytes, zam6218.o(i.__zam6218_read_data))
  [Stack]

  - Max Depth = 144
  - Call Chain = __zam6218_read_data ⇒ HAL_I2C_Mem_Read ⇒ I2C_RequestMemoryRead ⇒ I2C_WaitOnMasterAddressFlagUntilTimeout
  [Calls]
  - >> HAL_I2C_Mem_Read
  [Called By]
  - >> zam6218_get_temp

  __zam6218_reg_to_temp (Thumb, 70 bytes, Stack size 0 bytes, zam6218.o(i.__zam6218_reg_to_temp))
  [Called By]

  - >> zam6218_get_temp

  __zam6218_write_data (Thumb, 66 bytes, Stack size 40 bytes, zam6218.o(i.__zam6218_write_data))
  [Stack]

  - Max Depth = 144
  - Call Chain = __zam6218_write_data ⇒ HAL_I2C_Mem_Write ⇒ I2C_RequestMemoryWrite ⇒ I2C_WaitOnMasterAddressFlagUntilTimeout
  [Calls]
  - >> HAL_I2C_Mem_Write
  [Called By]
  - >> zam6218_config_set

  I2C_ConvertOtherXferOptions (Thumb, 28 bytes, Stack size 0 bytes, stm32f4xx_hal_i2c.o(i.I2C_ConvertOtherXferOptions))
  [Called By]

  - >> HAL_I2C_EV_IRQHandler

  I2C_DMAAbort (Thumb, 242 bytes, Stack size 24 bytes, stm32f4xx_hal_i2c.o(i.I2C_DMAAbort))
  [Stack]

  - Max Depth = 24
  - Call Chain = I2C_DMAAbort
  [Calls]
  - >> HAL_I2C_ErrorCallback
  - >> HAL_I2C_AbortCpltCallback
  [Address Reference Count : 2]
  - stm32f4xx_hal_i2c.o(i.I2C_ITError)
  - stm32f4xx_hal_i2c.o(i.I2C_Slave_STOPF)

  I2C_ITError (Thumb, 420 bytes, Stack size 24 bytes, stm32f4xx_hal_i2c.o(i.I2C_ITError))
  [Stack]

  - Max Depth = 24
  - Call Chain = I2C_ITError
  [Calls]
  - >> HAL_I2C_ListenCpltCallback
  - >> HAL_I2C_ErrorCallback
  - >> HAL_I2C_AbortCpltCallback
  - >> HAL_DMA_Abort_IT
  [Called By]
  - >> I2C_Slave_STOPF
  - >> HAL_I2C_ER_IRQHandler

  I2C_IsAcknowledgeFailed (Thumb, 62 bytes, Stack size 0 bytes, stm32f4xx_hal_i2c.o(i.I2C_IsAcknowledgeFailed))
  [Called By]

  - >> I2C_WaitOnTXEFlagUntilTimeout
  - >> I2C_WaitOnBTFFlagUntilTimeout

  I2C_MasterReceive_BTF (Thumb, 294 bytes, Stack size 16 bytes, stm32f4xx_hal_i2c.o(i.I2C_MasterReceive_BTF))
  [Stack]

  - Max Depth = 16
  - Call Chain = I2C_MasterReceive_BTF
  [Calls]
  - >> HAL_I2C_MemRxCpltCallback
  - >> HAL_I2C_MasterRxCpltCallback
  [Called By]
  - >> HAL_I2C_EV_IRQHandler

  I2C_MasterReceive_RXNE (Thumb, 226 bytes, Stack size 16 bytes, stm32f4xx_hal_i2c.o(i.I2C_MasterReceive_RXNE))
  [Stack]

  - Max Depth = 24
  - Call Chain = I2C_MasterReceive_RXNE ⇒ I2C_WaitOnSTOPRequestThroughIT
  [Calls]
  - >> I2C_WaitOnSTOPRequestThroughIT
  - >> HAL_I2C_MemRxCpltCallback
  - >> HAL_I2C_MasterRxCpltCallback
  - >> HAL_I2C_ErrorCallback
  [Called By]
  - >> HAL_I2C_EV_IRQHandler

  I2C_MasterTransmit_BTF (Thumb, 138 bytes, Stack size 16 bytes, stm32f4xx_hal_i2c.o(i.I2C_MasterTransmit_BTF))
  [Stack]

  - Max Depth = 16
  - Call Chain = I2C_MasterTransmit_BTF
  [Calls]
  - >> HAL_I2C_MasterTxCpltCallback
  [Called By]
  - >> HAL_I2C_EV_IRQHandler

  I2C_MasterTransmit_TXE (Thumb, 216 bytes, Stack size 24 bytes, stm32f4xx_hal_i2c.o(i.I2C_MasterTransmit_TXE))
  [Stack]

  - Max Depth = 40
  - Call Chain = I2C_MasterTransmit_TXE ⇒ I2C_MemoryTransmit_TXE_BTF
  [Calls]
  - >> I2C_MemoryTransmit_TXE_BTF
  - >> HAL_I2C_MemTxCpltCallback
  - >> HAL_I2C_MasterTxCpltCallback
  [Called By]
  - >> HAL_I2C_EV_IRQHandler

  I2C_Master_ADD10 (Thumb, 42 bytes, Stack size 0 bytes, stm32f4xx_hal_i2c.o(i.I2C_Master_ADD10))
  [Called By]

  - >> HAL_I2C_EV_IRQHandler

  I2C_Master_ADDR (Thumb, 616 bytes, Stack size 16 bytes, stm32f4xx_hal_i2c.o(i.I2C_Master_ADDR))
  [Stack]

  - Max Depth = 16
  - Call Chain = I2C_Master_ADDR
  [Called By]
  - >> HAL_I2C_EV_IRQHandler

  I2C_Master_SB (Thumb, 158 bytes, Stack size 0 bytes, stm32f4xx_hal_i2c.o(i.I2C_Master_SB))
  [Called By]

  - >> HAL_I2C_EV_IRQHandler

  I2C_MemoryTransmit_TXE_BTF (Thumb, 184 bytes, Stack size 16 bytes, stm32f4xx_hal_i2c.o(i.I2C_MemoryTransmit_TXE_BTF))
  [Stack]

  - Max Depth = 16
  - Call Chain = I2C_MemoryTransmit_TXE_BTF
  [Calls]
  - >> HAL_I2C_MemTxCpltCallback
  [Called By]
  - >> I2C_MasterTransmit_TXE
  - >> HAL_I2C_EV_IRQHandler

  I2C_RequestMemoryRead (Thumb, 348 bytes, Stack size 32 bytes, stm32f4xx_hal_i2c.o(i.I2C_RequestMemoryRead))
  [Stack]

  - Max Depth = 56
  - Call Chain = I2C_RequestMemoryRead ⇒ I2C_WaitOnMasterAddressFlagUntilTimeout
  [Calls]
  - >> I2C_WaitOnTXEFlagUntilTimeout
  - >> I2C_WaitOnMasterAddressFlagUntilTimeout
  - >> I2C_WaitOnFlagUntilTimeout
  [Called By]
  - >> HAL_I2C_Mem_Read

  I2C_RequestMemoryWrite (Thumb, 220 bytes, Stack size 32 bytes, stm32f4xx_hal_i2c.o(i.I2C_RequestMemoryWrite))
  [Stack]

  - Max Depth = 56
  - Call Chain = I2C_RequestMemoryWrite ⇒ I2C_WaitOnMasterAddressFlagUntilTimeout
  [Calls]
  - >> I2C_WaitOnTXEFlagUntilTimeout
  - >> I2C_WaitOnMasterAddressFlagUntilTimeout
  - >> I2C_WaitOnFlagUntilTimeout
  [Called By]
  - >> HAL_I2C_Mem_Write

  I2C_SlaveReceive_BTF (Thumb, 26 bytes, Stack size 0 bytes, stm32f4xx_hal_i2c.o(i.I2C_SlaveReceive_BTF))
  [Called By]

  - >> HAL_I2C_EV_IRQHandler

  I2C_SlaveReceive_RXNE (Thumb, 70 bytes, Stack size 16 bytes, stm32f4xx_hal_i2c.o(i.I2C_SlaveReceive_RXNE))
  [Stack]

  - Max Depth = 16
  - Call Chain = I2C_SlaveReceive_RXNE
  [Calls]
  - >> HAL_I2C_SlaveRxCpltCallback
  [Called By]
  - >> HAL_I2C_EV_IRQHandler

  I2C_SlaveTransmit_BTF (Thumb, 26 bytes, Stack size 0 bytes, stm32f4xx_hal_i2c.o(i.I2C_SlaveTransmit_BTF))
  [Called By]

  - >> HAL_I2C_EV_IRQHandler

  I2C_SlaveTransmit_TXE (Thumb, 70 bytes, Stack size 16 bytes, stm32f4xx_hal_i2c.o(i.I2C_SlaveTransmit_TXE))
  [Stack]

  - Max Depth = 16
  - Call Chain = I2C_SlaveTransmit_TXE
  [Calls]
  - >> HAL_I2C_SlaveTxCpltCallback
  [Called By]
  - >> HAL_I2C_EV_IRQHandler

  I2C_Slave_ADDR (Thumb, 102 bytes, Stack size 24 bytes, stm32f4xx_hal_i2c.o(i.I2C_Slave_ADDR))
  [Stack]

  - Max Depth = 24
  - Call Chain = I2C_Slave_ADDR
  [Calls]
  - >> HAL_I2C_AddrCallback
  [Called By]
  - >> HAL_I2C_EV_IRQHandler

  I2C_Slave_AF (Thumb, 156 bytes, Stack size 16 bytes, stm32f4xx_hal_i2c.o(i.I2C_Slave_AF))
  [Stack]

  - Max Depth = 16
  - Call Chain = I2C_Slave_AF
  [Calls]
  - >> HAL_I2C_SlaveTxCpltCallback
  - >> HAL_I2C_ListenCpltCallback
  [Called By]
  - >> HAL_I2C_ER_IRQHandler

  I2C_Slave_STOPF (Thumb, 386 bytes, Stack size 16 bytes, stm32f4xx_hal_i2c.o(i.I2C_Slave_STOPF))
  [Stack]

  - Max Depth = 40
  - Call Chain = I2C_Slave_STOPF ⇒ I2C_ITError
  [Calls]
  - >> I2C_ITError
  - >> HAL_I2C_SlaveRxCpltCallback
  - >> HAL_I2C_ListenCpltCallback
  - >> HAL_DMA_GetState
  - >> HAL_DMA_Abort_IT
  [Called By]
  - >> HAL_I2C_EV_IRQHandler

  I2C_WaitOnBTFFlagUntilTimeout (Thumb, 92 bytes, Stack size 16 bytes, stm32f4xx_hal_i2c.o(i.I2C_WaitOnBTFFlagUntilTimeout))
  [Stack]

  - Max Depth = 16
  - Call Chain = I2C_WaitOnBTFFlagUntilTimeout
  [Calls]
  - >> I2C_IsAcknowledgeFailed
  - >> HAL_GetTick
  [Called By]
  - >> HAL_I2C_Mem_Write

  I2C_WaitOnFlagUntilTimeout (Thumb, 134 bytes, Stack size 24 bytes, stm32f4xx_hal_i2c.o(i.I2C_WaitOnFlagUntilTimeout))
  [Stack]

  - Max Depth = 24
  - Call Chain = I2C_WaitOnFlagUntilTimeout
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> I2C_RequestMemoryWrite
  - >> I2C_RequestMemoryRead
  - >> HAL_I2C_Mem_Write
  - >> HAL_I2C_Mem_Read

  I2C_WaitOnMasterAddressFlagUntilTimeout (Thumb, 196 bytes, Stack size 24 bytes, stm32f4xx_hal_i2c.o(i.I2C_WaitOnMasterAddressFlagUntilTimeout))
  [Stack]

  - Max Depth = 24
  - Call Chain = I2C_WaitOnMasterAddressFlagUntilTimeout
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> I2C_RequestMemoryWrite
  - >> I2C_RequestMemoryRead

  I2C_WaitOnRXNEFlagUntilTimeout (Thumb, 128 bytes, Stack size 16 bytes, stm32f4xx_hal_i2c.o(i.I2C_WaitOnRXNEFlagUntilTimeout))
  [Stack]

  - Max Depth = 16
  - Call Chain = I2C_WaitOnRXNEFlagUntilTimeout
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> HAL_I2C_Mem_Read

  I2C_WaitOnSTOPRequestThroughIT (Thumb, 74 bytes, Stack size 8 bytes, stm32f4xx_hal_i2c.o(i.I2C_WaitOnSTOPRequestThroughIT))
  [Stack]

  - Max Depth = 8
  - Call Chain = I2C_WaitOnSTOPRequestThroughIT
  [Called By]
  - >> I2C_MasterReceive_RXNE

  I2C_WaitOnTXEFlagUntilTimeout (Thumb, 92 bytes, Stack size 16 bytes, stm32f4xx_hal_i2c.o(i.I2C_WaitOnTXEFlagUntilTimeout))
  [Stack]

  - Max Depth = 16
  - Call Chain = I2C_WaitOnTXEFlagUntilTimeout
  [Calls]
  - >> I2C_IsAcknowledgeFailed
  - >> HAL_GetTick
  [Called By]
  - >> I2C_RequestMemoryWrite
  - >> I2C_RequestMemoryRead
  - >> HAL_I2C_Mem_Write

  __NVIC_GetPriorityGrouping (Thumb, 10 bytes, Stack size 0 bytes, stm32f4xx_hal_cortex.o(i.__NVIC_GetPriorityGrouping))
  [Called By]

  - >> HAL_NVIC_SetPriority

  __NVIC_SetPriority (Thumb, 32 bytes, Stack size 8 bytes, stm32f4xx_hal_cortex.o(i.__NVIC_SetPriority))
  [Stack]

  - Max Depth = 8
  - Call Chain = __NVIC_SetPriority
  [Called By]
  - >> HAL_NVIC_SetPriority
  - >> HAL_SYSTICK_Config

  UART_DMAAbortOnError (Thumb, 20 bytes, Stack size 16 bytes, stm32f4xx_hal_uart.o(i.UART_DMAAbortOnError))
  [Stack]

  - Max Depth = 16
  - Call Chain = UART_DMAAbortOnError
  [Calls]
  - >> HAL_UART_ErrorCallback
  [Address Reference Count : 1]
  - stm32f4xx_hal_uart.o(i.HAL_UART_IRQHandler)

  UART_EndRxTransfer (Thumb, 54 bytes, Stack size 0 bytes, stm32f4xx_hal_uart.o(i.UART_EndRxTransfer))
  [Called By]

  - >> HAL_UART_IRQHandler

  UART_EndTransmit_IT (Thumb, 32 bytes, Stack size 8 bytes, stm32f4xx_hal_uart.o(i.UART_EndTransmit_IT))
  [Stack]

  - Max Depth = 8
  - Call Chain = UART_EndTransmit_IT
  [Calls]
  - >> HAL_UART_TxCpltCallback
  [Called By]
  - >> HAL_UART_IRQHandler

  UART_Receive_IT (Thumb, 190 bytes, Stack size 16 bytes, stm32f4xx_hal_uart.o(i.UART_Receive_IT))
  [Stack]

  - Max Depth = 16
  - Call Chain = UART_Receive_IT
  [Calls]
  - >> HAL_UART_RxCpltCallback
  - >> HAL_UARTEx_RxEventCallback
  [Called By]
  - >> HAL_UART_IRQHandler

  UART_SetConfig (Thumb, 546 bytes, Stack size 40 bytes, stm32f4xx_hal_uart.o(i.UART_SetConfig))
  [Stack]

  - Max Depth = 80
  - Call Chain = UART_SetConfig ⇒ __aeabi_uldivmod
  [Calls]
  - >> HAL_RCC_GetPCLK2Freq
  - >> HAL_RCC_GetPCLK1Freq
  - >> __aeabi_uldivmod
  [Called By]
  - >> HAL_UART_Init

  UART_Transmit_IT (Thumb, 96 bytes, Stack size 0 bytes, stm32f4xx_hal_uart.o(i.UART_Transmit_IT))
  [Called By]

  - >> HAL_UART_IRQHandler

  UART_WaitOnFlagUntilTimeout (Thumb, 108 bytes, Stack size 24 bytes, stm32f4xx_hal_uart.o(i.UART_WaitOnFlagUntilTimeout))
  [Stack]

  - Max Depth = 24
  - Call Chain = UART_WaitOnFlagUntilTimeout
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> HAL_UART_Transmit

  _fp_digits (Thumb, 366 bytes, Stack size 64 bytes, printfa.o(i._fp_digits), UNUSED)
  [Calls]

  - >> __aeabi_dmul
  - >> __aeabi_ddiv
  - >> __aeabi_dadd
  - >> __aeabi_d2ulz
  - >> __aeabi_cdrcmple
  - >> __aeabi_uldivmod
  [Called By]
  - >> _printf_core

  _printf_core (Thumb, 1744 bytes, Stack size 136 bytes, printfa.o(i._printf_core), UNUSED)
  [Calls]

  - >> __aeabi_uidivmod
  - >> _printf_pre_padding
  - >> _printf_post_padding
  - >> _fp_digits
  - >> __aeabi_uldivmod
  [Called By]
  - >> __0sprintf

  _printf_post_padding (Thumb, 36 bytes, Stack size 24 bytes, printfa.o(i._printf_post_padding), UNUSED)
  [Called By]

  - >> _printf_core

  _printf_pre_padding (Thumb, 46 bytes, Stack size 24 bytes, printfa.o(i._printf_pre_padding), UNUSED)
  [Called By]

  - >> _printf_core

  _sputc (Thumb, 10 bytes, Stack size 0 bytes, printfa.o(i._sputc))
  [Called By]

  - >> __0sprintf
  [Address Reference Count : 1]
  - printfa.o(i.__0sprintf)

  ### Undefined Global Symbols