Reporting Options

# File in Previous Format

Date | : | 2023/3/21
Time | : | 17:37:27
Filename | : | D:\F\ZSN603读卡专用芯片\3.硬件设计\【硬件设计】基于ZSN603的读卡模块设计资料\ZSN603-EVK3 Rev.A_LT2\ZSN603-EVK3 Rev.A.PcbDoc

Version | Warning
--- | ---
Altium Designer update 19 | CAUTION - Air Gap Width attribute was introduced to Polygon Connect Style Rule. Air Gap Width attribute now controls the distance between poured polygon and pads on the same net - this value was previosuly taken from clearance rule while ignoring net subscope leading to sometime unexpected results.
Release 13 | CAUTION - Silkscreen Over Component Pads Rules are converted to Silk To Solder Mask Clearance Rules. Suggest examining rule scopes for accuracy.
Release 14 | CAUTION - The Differential Pairs Routing rule added support for control of the width. Be aware that Width rules pertaining to differential pairs need to be manually moved to the Differential Pairs Routing rule.

This file was generated by an earlier version of the software